|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CONDITION OF SALE / SPECIAL INSTRUOCTINS:  This will be provided under separate cover. | | | |  | Quotation | |
| PRODUCT: OXYGEN CONCENTRATORS - 5L & 10L | APPLICATION: Medical | | | |
| SALESPERSON | P.O. NUMBER | SHIP DATE |  | SHIP VIA | F.O.B. POINT | DELIVERY TERMS |
| Gerald Provost | TO BE PROVIDED | TBD |  | BUYER LOGISTICS | China: Outgoing port could be  Shanghai, Shenzhen,  GuanZhou or Hong Kong. | PER CUSTOMER |
|  | | | |  |  | |
| QUANTITY | DESCRIPTION | | PACKAGING | UNIT PRICE | IMAGE |  |
| 2000 | 5L Stationary Oxygen Concentrator  Capacity : 5 L  Purity Oxygen: ≥ 93%±3 ( V/V ) Flow rate: 1-5L/min Voltage:  AC220V±22V,50Hz±1Hz/AC110V±15  V,60Hz±1Hz  Output Pressure: 20kPa～60kPa  Sound Level: less than 45db  Power Consumption: 300watts  Guarantee: 12 months  Gross Weight：25kg  Package Size：55\*33\*65 |  CERTIFICATION  CE | FDA | ISO13485 | | MOQ: N/A  Lead Time: 3-5 days Accessories included:  1 x Oxygen Concentrator   1. x Humidifier Bottle 2. x Nasal oxygen cannula   2 x First Filter  6 x Second Filter  1 x User Manual  1 x Warranty Card | $799.00 | FWB-WMC-01 |  |
| 2000 | 5L Stationary Oxygen Concentrator  Capacity : 5 L  Purity Oxygen: ≥ 93%±3（V/V）  Flow rate:1-5L/min  Voltage：  AC220V±22V,50Hz±1Hz/AC110V±15  V,60Hz±1Hz  Output Pressure：20kPa～60kPa  Sound Level: less than 45db power  Consumption: 300VA  Gross Weight: 23kg  Package Size：44\*39\*69c CERTIFICATION  CE | FDA | ISO13485 | | MOQ: N/A  Lead Time: 3-5 days Accessories included:  1 x Oxygen Concentrator   1. x Humidifier Bottle 2. x Nasal oxygen cannula   1 x First Filter  1 x HEPA Filter  1 x User Manual | $834.40 | FWB-WMC-02 |  |
| 2000 | 5L Stationary Oxygen Concentrator  Capacity : 5 L  Purity Oxygen: ≥ 93%±3（V/V） Flow rate: 1-5L/min Voltage：  AC220V±22V,50Hz±1Hz/AC110V±15  V,60Hz±1Hz  Output Pressure：20kPa～60kPa  Sound Level: less than 45db  Power Consumption: 300VA  Gross Weight: 23kg  Package Size：44\*39\*69cm  CERTIFICATION  CE | FDA | ISO13485 | | MOQ: N/A  Lead Time: 3-5 days Accessories included:  1 x Oxygen Concentrator   1. x Humidifier Bottle 2. x Nasal oxygen cannula   1 x First Filter  1 x HEPA Filter  1 x User Manual | $858.00 | FWB-WMC-03 |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 2000 | 10L Stationary Oxygen Concentrator  Capacity : 10 L  Purity Oxygen: ≥ 93%±3（V/V）  Flow Rate: 1-10L/min  Voltage：  AC220V±22V,50Hz±1Hz/AC110V±15  V,60Hz±1Hz  Output Pressure：20kPa～60kPa  Sound Level: less than 48db  Power Consumption: 550VA  Gross Weight: 28kg  Package Size：44\*39\*73cm  CERTIFICATION  CE | FDA | ISO13485 | MOQ: N/A  Lead Time: 3-5 days Accessories included:  1 x Oxygen Concentrator   1. x Humidifier Bottle 2. x Nasal oxygen cannula   1 x First Filter  1 x HEPA Filter  1 x User Manual | $1021.40 | FWB-WMC-04 |  |
| 1000 | 10L Stationary Oxygen Concentrator  Capacity : 10 L  Purity Oxygen: ≥ 93%±3（V/V）  Flow Rate: 1-10L/min  Voltage：  AC220V±22V,50Hz±1Hz/AC110V±15 V,60Hz±1Hz  Output Pressure：20kPa～60kPa  Sound Level: less than 48db  Power Consumption: 550VA  Gross Weight: 28kg  Package Size：44\*39\*73c  CERTIFICATION  CE | FDA | ISO13485 | MOQ: N/A  Lead Time: 3-5 days Accessories included:  1 x Oxygen Concentrator   1. x Humidifier Bottle 2. x Nasal oxygen cannula   2 x First Filter  6 x Second Filter  1 x User Manual  1 x Warranty Card | $1070.40 |  |  |
|  |  |  |  |  |  |
|  | | | | |  |
|  |
|  |
|  |
|  |
| THANK YOU  FOR YOUR BUSINESS |
|  | | | | | |
| ENDORSEMENTS  PROSPECTIVE CUSTOMER    Name  Managing Principal Title | | | | | |